R1>en

R1#conf t

Enter configuration commands, one per line. End with CNTL/Z.

R1(config)#int g0/0

R1(config-if)#ip help

R1(config-if)#ip helper-address 192.168.60.253

R1(config-if)#

Cisco Packet Tracer PC Command Line 1.0

C:\>ping 209.165.202.158

Pinging 209.165.202.158 with 32 bytes of data:

Request timed out.

Reply from 209.165.202.158: bytes=32 time=2ms TTL=125

Reply from 209.165.202.158: bytes=32 time=5ms TTL=125

Reply from 209.165.202.158: bytes=32 time=7ms TTL=125

Ping statistics for 209.165.202.158:

Packets: Sent = 4, Received = 3, Lost = 1 (25% loss),

Approximate round trip times in milli-seconds:

Minimum = 2ms, Maximum = 7ms, Average = 4ms

C:\>ping 209.165.202.157

Pinging 209.165.202.157 with 32 bytes of data:

Request timed out.

Reply from 209.165.202.157: bytes=32 time=1ms TTL=125

Reply from 209.165.202.157: bytes=32 time=5ms TTL=125

Reply from 209.165.202.157: bytes=32 time=1ms TTL=125

Ping statistics for 209.165.202.157:

Packets: Sent = 4, Received = 3, Lost = 1 (25% loss),

Approximate round trip times in milli-seconds:

Minimum = 1ms, Maximum = 5ms, Average = 2ms